From 8dd092ba32ba1b29a3ce74b3031f85e9d9b91caf Mon Sep 17 00:00:00 2001
From: Blaise Thompson <blaise@untzag.com>
Date: Fri, 16 Apr 2021 08:40:15 -0500
Subject: pcb assembly pictures

---
 assembly-instructions/wpr-assembly.tex | 29 ++++++++++++++++++++++++-----
 1 file changed, 24 insertions(+), 5 deletions(-)

(limited to 'assembly-instructions/wpr-assembly.tex')

diff --git a/assembly-instructions/wpr-assembly.tex b/assembly-instructions/wpr-assembly.tex
index f41885d..075eeed 100644
--- a/assembly-instructions/wpr-assembly.tex
+++ b/assembly-instructions/wpr-assembly.tex
@@ -140,18 +140,35 @@ More details about this digital control system are in TODO: LINK TO SECTION.
 \clearpage
 \subsection{Analog}
 
-TODO: PICTURE OF PCB AS DELIVERED BY MANUFACTURER
+\begin{center}
+  \includegraphics[width=\textwidth/2]{"./bare-pcb.jpg"}
+\end{center}
+
+\begin{center}
+  \includegraphics[width=\textwidth/2]{"./surface-mount.jpg"}
+\end{center}
 
-TODO: ADD SURFACE MOUNT
 Recommend thin solder, e.g. 0.015''.
 Small green line on LED towards ground (left).
 
-TODO: ADD CONNECTORS, TRIMPOT
+\begin{center}
+  \includegraphics[width=\textwidth/2]{"./connectors.jpg"}
+\end{center}
+
 Recommend standard solder, e.g. 0.031''.
 
-TODO: ADD BARREL JACKS, TEST POINTS
+\begin{center}
+  \includegraphics[width=\textwidth/2]{"./connectors.jpg"}
+\end{center}
+
+\begin{center}
+  \includegraphics[width=\textwidth/2]{"./barrels-tested.jpg"}
+\end{center}
+
+\begin{center}
+  \includegraphics[width=\textwidth/2]{"./pcb-driver.jpg"}
+\end{center}
 
-TODO: TEST
 150 mA to 3 V
 
 TODO: ADD DRIVER
@@ -184,6 +201,8 @@ Add lead-based solder to make easier
 
 TODO: LED PCB part number
 
+TODO: LED PINS SOLUTION
+
 TODO: heatsink part number
 
 \begin{center}
-- 
cgit v1.2.3

