From 80baee9f019af151743b3d6e49cddaa44656ac7d Mon Sep 17 00:00:00 2001
From: Blaise Thompson <blaise@untzag.com>
Date: Sat, 7 Apr 2018 18:20:04 -0500
Subject: 2018-04-07 18:20

---
 abstract.tex | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

(limited to 'abstract.tex')

diff --git a/abstract.tex b/abstract.tex
index c9c8d9e..64d230f 100644
--- a/abstract.tex
+++ b/abstract.tex
@@ -16,7 +16,7 @@ This approach has several unique capabilities:
 \end{denumerate}
   
 CMDS can be collected in the frequency or the time domain, and each approach has advantages and
-disadvantages.  %
+disadvantages. \cite{ParkKisam1998a}  %
 Frequency domain ``Multi-resonant'' CMDS (MR-CMDS) requires pulsed ultrafast light sources with
 tunable output frequencies.  %
 These pulses are directed into a material under investigation.  %
-- 
cgit v1.2.3

