From 1b66cf20d0f40741d89d39b901716341beeabeca Mon Sep 17 00:00:00 2001
From: Blaise Thompson <blaise@untzag.com>
Date: Mon, 16 Oct 2017 21:05:20 -0500
Subject: structure

---
 appendix/hardware.tex | 34 ----------------------------------
 1 file changed, 34 deletions(-)
 delete mode 100644 appendix/hardware.tex

(limited to 'appendix/hardware.tex')

diff --git a/appendix/hardware.tex b/appendix/hardware.tex
deleted file mode 100644
index c69d7e9..0000000
--- a/appendix/hardware.tex
+++ /dev/null
@@ -1,34 +0,0 @@
-\chapter{Hardware}  % -----------------------------------------------------------------------------
-
-
-\section{Adjustable periscopes}  % ----------------------------------------------------------------
-
-
-Our light sources take on horizontal or vertical polarizations according to which tuning process is
-used.  %
-Our experiments are opinionated about polarization, so some strategy for aligning polarization is
-necessary.  %
-Desire fully reflective, easy to switch without changing path length (delay) etc... For several
-years, we used brewster-angle polarization unifiers...  %
-These worked by...  %
-But these were very difficult to align, and they were too lossy for some of the weaker tuning
-processes.  %
-As an alternative, we designed a more traditional periscope with adjustability for our unique
-needs.  %
-
-
-\subsection{Alignment}  % -------------------------------------------------------------------------
-
-
-\begin{enumerate}
-  \item in flipped polarization:
-    \begin{itemize}
-      \item stage near
-      \item upper mirror far
-    \end{itemize}
-  \item in kept polarization:
-    \begin{itemize}
-      \item stage x and upper mirror height near
-      \item lower mirror far
-    \end{itemize}
-\end{enumerate}
-- 
cgit v1.2.3

