From 4ddc0bcecdd172e6fbed0df2e80dfc7663b6ab73 Mon Sep 17 00:00:00 2001
From: Blaise Thompson <blaise@untzag.com>
Date: Sun, 12 Nov 2017 18:51:13 -0600
Subject: structure

---
 hardware.tex | 37 -------------------------------------
 1 file changed, 37 deletions(-)
 delete mode 100644 hardware.tex

(limited to 'hardware.tex')

diff --git a/hardware.tex b/hardware.tex
deleted file mode 100644
index b5a02d7..0000000
--- a/hardware.tex
+++ /dev/null
@@ -1,37 +0,0 @@
-\chapter{Hardware}  % -----------------------------------------------------------------------------
-
-
-\section{Adjustable periscopes}  % ----------------------------------------------------------------
-
-
-Our light sources take on horizontal or vertical polarizations according to which tuning process is
-used.  %
-Our experiments are opinionated about polarization, so some strategy for aligning polarization is
-necessary.  %
-Desire fully reflective, easy to switch without changing path length (delay) etc... For several
-years, we used brewster-angle polarization unifiers...  %
-These worked by...  %
-But these were very difficult to align, and they were too lossy for some of the weaker tuning
-processes.  %
-As an alternative, we designed a more traditional periscope with adjustability for our unique
-needs.  %
-
-\begin{figure}[htp!]
-	\centering
-	\includegraphics[scale=0.1]{"hardware/periscope"}
-	\label{f:periscope}
-	\caption{CAPTION TODO}
-\end{figure}
-
-\begin{enumerate}
-  \item in flipped polarization:
-    \begin{itemize}
-      \item stage near
-      \item upper mirror far
-    \end{itemize}
-  \item in kept polarization:
-    \begin{itemize}
-      \item stage x and upper mirror height near
-      \item lower mirror far
-    \end{itemize}
-\end{enumerate}
-- 
cgit v1.2.3

