From 3bc8b4451803929d6a47f87a987947c37d95545d Mon Sep 17 00:00:00 2001
From: Blaise Thompson <blaise@untzag.com>
Date: Thu, 12 Apr 2018 21:00:37 -0500
Subject: 2018-04-12 21:00

---
 opa/chapter.tex | 10 +++++-----
 1 file changed, 5 insertions(+), 5 deletions(-)

(limited to 'opa/chapter.tex')

diff --git a/opa/chapter.tex b/opa/chapter.tex
index 59e4243..89d4d5d 100644
--- a/opa/chapter.tex
+++ b/opa/chapter.tex
@@ -16,15 +16,15 @@
 \section{Introduction}  % =========================================================================
 
 In frequency-domain Multi-Resonant Coherent Multidimensional Spectroscopy (MR-CMDS), automated
-Optical Parametric Amplifiers (OPAs) are used to actively scan excitation color axes. %
-To accomplish these experiments, exquisite OPA performance is required. %
+Optical Parametric Amplifiers (OPAs) are used to actively scan excitation color axes. [CITE]  %
+To accomplish these experiments, exquisite OPA performance is required.  %
 During the experiment, motors inside the OPA move to pre-recorded positions to optimize output at
-the desired color. %
+the desired color.  %
 Parametric conversion (``mixing'') strategies are now readily avalible, extending the 800 nm pumped
-OPA tuning range into the visible, near-infrared, and mid-infrared. %
+OPA tuning range into the visible, near-infrared, and mid-infrared.  %
 
 OPAs are very sensitive to changes in upstream lasers and lab conditions, so OPA tuning is
-regularly required. %
+regularly required.  %
 Manual OPA tuning can easily take a full day. %
 Furthermore, manual tuning typically results in inferior tuning curves, since it is difficult to
 consider all available information simultaneously.  %
-- 
cgit v1.2.3

