From 798bd484137439bf1d0752ddde82bf49da4af6b7 Mon Sep 17 00:00:00 2001
From: Blaise Thompson <blaise@untzag.com>
Date: Mon, 16 Apr 2018 13:32:20 -0500
Subject: 2018-04-16 13:32

---
 opa/chapter.tex | 9 +++++----
 1 file changed, 5 insertions(+), 4 deletions(-)

(limited to 'opa/chapter.tex')

diff --git a/opa/chapter.tex b/opa/chapter.tex
index db88304..00e3203 100644
--- a/opa/chapter.tex
+++ b/opa/chapter.tex
@@ -121,7 +121,7 @@ After the poweramp, the output signal and idler can be sent through appropriate
 optionally, mixed further in three subsequent mixing stages to create all of the ranges seen in
 \autoref{opa:fig:ranges}.  %
 Each of these mixing stages has only crystal angle tunability.  %
-I describe my strategy for mixer tuning in \autoref{opa:sec:mixer}.  %
+I describe my strategy for mixer tuning in \autoref{opa:sec:mixers}.  %
 
 It is important to realize that the total conversion efficiency for each output color varies wildly
 over all of the different mixing strategies.  %
@@ -180,7 +180,8 @@ I then search along that contour in \emph{intensity} space to find the motor pos
 maximum intensity for that color.  %
 Finally I fit a smooth spline through those chosen values to generate the output curve.  %
 
-A representative preamp tune procedure output image is shown in \autoref{fig:autotune_preamp}.  %
+A representative preamp tune procedure output image is shown in
+\autoref{opa:fig:autotune_preamp}.  %
 This is an automatically generated image from PyCMDS.  %
 The thick black line is the final output curve.  %
 The dark grey lines are the contours of constant color.  %
@@ -233,14 +234,14 @@ dimensions (this is especially true at the edge output colors).  %
 In the poweramp, the increased dimensionaity makes it too expensive to do a full multidimensional
 tuning procedure.  %
 Instead we emply an iterative procedure as diagrammed below.  %
-\autoref{fig:opa:poweramp_flowchart} diagrams this iterative procedure.  %
+\autoref{opa:fig:poweramp_flowchart} diagrams this iterative procedure.  %
 
 We always end the iteration(s) with C2 so that the OPA's color calibration is as good as
 possible.  %
 Typically only one iteration is required but multiple iterations may be necessary if dramatic OPA
 realignment has occurred.  %
 In total, poweramp tuning typically takes less than 1 hour. %
-Representative procedure output images for D2 (\autoref{op:fig:d2}) and C2 (\autoref{opa:fig:c2})
+Representative procedure output images for D2 (\autoref{opa:fig:d2}) and C2 (\autoref{opa:fig:c2})
 are shown.  %
 
 For the D2 figure, the lower panel shows the intensity of the data taken.  %
-- 
cgit v1.2.3

