From b75d9d8f2ba798fbbadc975a789cf2615b743328 Mon Sep 17 00:00:00 2001
From: Blaise Thompson <blaise@untzag.com>
Date: Sun, 15 Apr 2018 00:16:26 -0500
Subject: 2018-04-15 00:16

---
 procedures/chapter.tex | 49 +++++++++++++++++++++++--------------------------
 1 file changed, 23 insertions(+), 26 deletions(-)

(limited to 'procedures/chapter.tex')

diff --git a/procedures/chapter.tex b/procedures/chapter.tex
index fd04bc3..8c8d0b2 100644
--- a/procedures/chapter.tex
+++ b/procedures/chapter.tex
@@ -1,7 +1,17 @@
 \chapter{Procedures}
 
-\clearpage
-\section{``Six-month'' maintenance}  % ------------------------------------------------------------
+\begin{dquote}
+  These are the vegetables we must eat before we can have our pixels of ice cream.
+
+  \dsignature{Wright Group saying}.
+\end{dquote}
+
+\vfill
+
+In this chapter I document the various procedures that I have performed to maintain the MR-CMDS
+instruments.  %
+
+\section{``Six-month'' maintenance}  % ============================================================
 
 The laser system that the Wright Group's MR-CMDS instruments use requires regular maintenance.  %
 Each component is sensitive to lab conditions such as temperature, humidity, and vibrations.  %
@@ -13,7 +23,6 @@ Historically, the Wright Group has engaged in reactive maintenance: a ``fix it i
 don't touch otherwise'' kind of approach.  %
 This approach makes a lot of sense for instruments that are quick to fix, and have few active
 users.  %
-
 I instituted a proactive, regular maintenance procedure (described below) that has improved the
 predictability of instrumental performance.  %
 Predictability is key for instruments with multiple users.  %
@@ -48,9 +57,9 @@ Procedure:
         \end{denumerate}
       \item Chiller maintenance.
         \begin{ditemize}
-          \item See x
-          \item See y
-          \item See z
+          \item See \autoref{prc:sec:lytron}
+          \item See \autoref{prc:sec:polyscience}
+          \item See \autoref{prc:sec:neslab}
         \end{ditemize}
       \item Lab cleaning.
         \begin{denumerate}
@@ -68,13 +77,9 @@ Procedure:
     \end{ditemize}
   \item Let lab sit overnight to allow dust to settle and the air to dehumidify.
   \item Start up system again.
-    \begin{denumerate}
-      \item TODO
-    \end{denumerate}
 \end{denumerate}
 
-\clearpage
-\section{Lytron Kodiak RC006}  % ------------------------------------------------------------------
+\section{Lytron Kodiak RC006} \label{prc:sec:lytron}  % ===========================================
 
 We have one Lytron Kodiak RC006: Model Number RC006G03BB1C002, Serial Number 739383-02.
 
@@ -107,10 +112,7 @@ These seem to have been fixed by adding a “high” flow loop connecting the ou
 chiller.  %
 Ideally the pressure drop across this loop is sufficient to still drive fluid through the laser.  %
 
-% TODO: figure
-
-\clearpage
-\section{PolyScience 6000 Series}  % --------------------------------------------------------------
+\section{PolyScience 6000 Series} \label{prc:sec:polyscience}  % ==================================
 
 We own two PolyScience chillers---different models but functionally equivalent.
 
@@ -142,8 +144,7 @@ Regular chiller maintenance:
     \end{denumerate}
 \end{denumerate}
 
-\clearpage
-\section{NesLab Merlin M33}  % ====================================================================
+\section{NesLab Merlin M33} \label{prc:sec:neslab}  % =============================================
 
 We have one NesLab Merlin M33 Chiller, Serial Number 106227049.  %
 
@@ -171,7 +172,6 @@ Regular chiller maintenance
 
 % TODO: figures
 
-\clearpage
 \section{Calibrating the 407A}  % =================================================================
 
 Calibrating the 407.A
@@ -180,11 +180,11 @@ You may sometimes notice that the zero position changes dramatically from sensit
 sensitivity with the 407A. If this happens, iterate through the following until zero stays
 consistent:
 
-Use the fine adjust (knob on side) to zero the 407A on the highest sensitivity
-
-Use the front adjust (flathead screwdriver needed) to zero on the lowest sensitivity
-
-\clearpage
+\begin{ditemize}
+  \item Use the fine adjust (knob on side) to zero the 407A on the highest sensitivity.
+  \item Use the front adjust (flathead screwdriver needed) to zero on the lowest sensitivity.
+\end{ditemize}
+    
 \section{Millenia}  % =============================================================================
 
 \subsection{Startup}  % ---------------------------------------------------------------------------
@@ -228,7 +228,6 @@ These allow us to record things like Diode hours.  %
 Service mode can be buggy, so it's best to leave the Millenia in normal Power mode during regular
 operation.  %
 
-\clearpage
 \section{Spitfire Pro}  % =========================================================================
 
 Only tune up the Spitfire if you need to, and do not treat it casually---set aside an entire
@@ -429,7 +428,6 @@ Since we have not messed with the stretcher frequently this guide cannot be trus
     square mirrors preceding the compressor.
 \end{denumerate}
   
-\clearpage
 \section{TOPAS-C}  % ==============================================================================
 
 % TODO: figure
@@ -668,7 +666,6 @@ Input poynting is adjusted to ensure good alignment through L1 and L2 into D1.
   \item Measure and record power---should be over 600 mW.
 \end{denumerate}
 
-\clearpage
 \section{MicroHR Monochromator}  % ================================================================
 
 Visible Grating.  %
-- 
cgit v1.2.3

